H & H Technical, LLC

1949 Sugarland Dr. Ste. 134

Sheridan, Wyoming 82801

Phone (307) 672-0743	hdts@wavecom.net	Fax (307) 672-5118

Quote 877 rev 4 Gas Compressor

Jan. 1, 2011

Mr.Jerry Tan

Director

Logistic Technical Supply Pte. Ltd.,

160 Choa Chu Kang Ave. 1

Singapore 689450

Dear Mr.Tan

H&H Technical, LLC is pleased to offer for your consideration the following:

- (1) Newly packaged Ariel JGH/4-3 compressor driven by a Caterpillar 3516 LE engine.

-(1) Instruments and controls needed to install a minium and maximum suction control system on the above listed compressor .

The investment required to purchase this unit is $1,065,113.00 per the attached Equipment specifications and Conditions of Sale. Delivery will be 18 to 22 weeks after receipt of down payment.

This quote is based on the gas conditions shown on page two of this quote.

Quote is only good for 60 days.

If you have any questions please call or fax.

Thank you,

Mike Harkins

Design Conditions

Suction Pressure (psig)………………………………	10

Discharge Pressure (psig)…………………………….	450

Flow (MMSCF/D)……………………………………	4.506

Inlet Temperature (deg. F)……………………….….	80

Aftercooling Gas (deg. F)…..…….…………………	120

Elevation (ft.)………………………………………	100

Specific Gravity……………………………………..	.81

Ambient Temperature (deg. F)………………………	100

Skid

Packager is Natural Gas Compression Systems, Inc. ("NGCS")

NGCS starts with a solid foundation consisting of four structural steel main I-beam runners with thoroughly welded interconnecting I-beams to support the engine base, compressor base, scrubbers, panel board, cooler, and pipe supports/hold downs. This allows for proper support and foundation. Skids are covered with diamond decking steel plate with concrete fill in critical skid sections. Each end includes a tail-roll and lifting eyes. A two-inch pollution rail surrounds the skid and drains are also provided. NGCS builds a very robust skid and believes this is critical to constructing a well running compressor package.

Compressor

JGH 4 throw 4 stage compressor package cylinders as follows:

Design	Balanced/ Opposed

Drive	Direct Connected

1st stage	2nd stage	3rd stage

Number of cylinders	(2)	(1)	(1)

Cylinder	17.250"	13.000"	8.000"

MAWP	230 psig	300 psig	800 psig

Material	Ductile Iron	Ductile Iron	Ductile Iron

Rod Load (total)	48,000	48,000	48,000

Variable Volume Pkt.	Yes	Yes	Yes

Engine

Manufacturer:	Caterpillar

Model:	3516 LE AFRC

RATED:	1150 HP @ 1200 rpm

Engine and starting accessories

NGCS's Standard Caterpillar Engine Configuration includes:

Governor, Woodward Electronic actuator with 2301A control

Turbine-type Starter

Fisher fuel gas regulator

Fuel gas relief valve set for protection of regulator

Hospital grade muffler

Expansion joint – wrinkle belly

Exhaust pipe

Pre/post lube

Fuel gas filter

Adem III Ignition System

Cooler

R & R Engineering Cooler Model UI -12-24Y, vertical coil, horizontal intake, vertical discharge single fan forced draft, engine driven air cooled heat exchanger complete with Moore Class 10000 VT Low Noise Fan; sheaves guards, ASME cod stamped design, manual louvers on gas sections. The cooler is designed based on 100 degree F ambient with a 20 degree F approach.

Qty	Service	Discharge Temp	MAWP

1	EJW	165 F	150 psig @ 300 F

1	TAW	130 F	150 psig @ 300 F

1	IC1	120 F	150 psig @ 300 F

1	IC2	120 F	300 psig @ 300 F

1	After Cooler	120 F	600 psig @ 300 F

Cooler will be painted primer red.

Scrubbers

One (1) Inlet filter scrubber and one (2) interstage scrubber. Scrubbers are ASME code stamped and are vertically skirt mounted on structural steel members.

Each scrubber is complete with the following:

-High-level shutdown switch Murphy Control 1200 series.

-Automatic liquid level controller and dump valve – Kimray

-Manual drains

-Each dump valve is isolated for repairs if necessary while unit is running

-Gauge glass w/cocks

Control Panel

Altronic control panel in a weatherproof enclosure with a freestanding base, removable rear door and a hinged front door with safety glass window and shock mounted inner panel. The annunciator includes an adjustable start-up timer, stop switch and test mode. Annunciator will scan end devices for faults before start-up. First cause of shutdown is displayed on LCD readout and retained in memory. Panel is complete with the following:

Shutdowns:	Panel Mounted Gauges:

Low Engine Oil Pressure	Suction Pressure – each stage

Low engine Oil Level	Discharge Pressure – each stage

Low Engine Coolant Level	Compressor Oil pressure

High Coolant Temperature

High Engine Oil Temperature	Tachometer//Hour Meter

Overspeed	Engine Oil Pressure

Engine Vibration	Engine Jacket Water Temperature

Low Compressor Oil Pressure	Auxiliary Water discharge Temperature

Low Compressor Oil Level	Oil Temperature

Lubricator No Flow	Manifold Pressure

High Compressor Oil Temperature

Compressor Vibration	0-5 Minute Start – Run Timer

Cooler Vibration	Stop- Run Switch

Low Suction Pressure – each stage	Push to start

High Suction Pressure- each stage

Low Discharge Pressure – each stage

High Discharge Pressure – each stage

High Discharge Temperature –each stage

High Scrubber Liquid Level – each stage

Emergency Stop

Relief Valves

Anderson Greenwood

Accessory Equipment

Coupling and Coupling Guard

Relief valve is included on the discharge

Estimated Package Dimensions

Engine & Compressor	13.5' W x 40' L x 11' H

Weight	100,000 lbs.

Cooler	23'6" L x 13' 6" H x 8'6" D

Weight	29,000 lbs.

Engineering

General arrangement drawing	(qty. 3)

Elevations views	(qty. 3)

Process flow diagrams	(qty. 3)

Utility diagrams	(qty. 3)

Panel drawings	(qty. 3)

Operation & Maintenance manuals	(qty. 3)

Att: Mr. Jerry Tan

Subject: Agreement for Sale

Mr. Tan:

The attached agreement sets forth the terms and conditions governing the sale, by H&H Technical, LLC of the equipment and services listed in the attached quotation.

Conditions of Sale, Material Balance, and Equipment Specifications are included in the attached quotation and are part of this agreement.

This agreement is made and entered into on, or around ____________, 2010

For the Purchaser:

_____________________________________	_______________

Mr. Jerry Tan	Date

Logistic Technical Supply Pte. Ltd.

For H&H Technical, LLC:

____________________________________	_______________

Mike Harkins	Date

____________________________________	_______________

Brian Hamilton	Date

CONDITIONS OF SALE

I.	CONDITIONS:

(A)	No terms of conditions contained in any order placed with H & H Technical LLC other than those stated herein shall be binding on H & H Technical LLC, unless hereafter agreed to in writing.

(B)	All orders are subject to acceptance by an officer of H & H Technical LLC.

II.	PRICES:

(A)	Prices quoted are EXW our shop in Sheridan, Wyoming, or our vendors shop, exclusive of any sales or use taxes, and are payable in U.S. dollars.

(B)	Prices quoted are firm for acceptance within 60-days of the date quoted.

III. TERMS OF PAYMENT:

(A)	Thirty percent (30%) of quoted price, which equals $319,534.00, will be submitted within 30 days of purchase order, letter of intent, or written authorization to proceed.

(B)	The balance will be paid as follows:

(1) Thirty percent (30%) of the quoted price, which is $319,534.00, is due upon vendors receipt of Ariel Compressor. At this time, that is estimated to be 12 weeks after placing of order by customer and payment of down payment.

(2)Thirty percent (30%) of the quoted price, which is $319,534.00, is due upon vendors receipt of Cat Engine. At this time, that is estimated to be 18 weeks after placing of order by customer and payment of down payment.

(3) Final ten percent (10%) of the quoted price, which is $106,511.00, is due prior shipment of unit. At this time, that is estimated to be 18 to 22 weeks after placing of order by customer and payment of down payment.

(C)	If shipment is prevented or postponed at the purchaser's request, then all dates of payment relating to shipment shall relate instead to the date of completion. Storage of such machinery will be at the purchaser's expense and risk.

(D)	Service charges will be assessed on delinquent accounts at the rate of 1.5% per month.

(E)	All orders are subject to approval of credit.

(F)	All monies shall be wired transferred by the designated times to the following address:

H & H Technical LLC

1949 Sugarland Drive, Suite 134

Sheridan, Wyoming 82801

USA

In care of:

First Interstate Bank

1613 South Coffeen Avenue,

Sheridan, Wyoming 82801

Routing No. 092901683

Accounting No. 0201145570

IV.	WARRANTY:

H & H Technical LLC ("The Company") warrants the equipment of its manufacture to be delivered hereunder against defects in material and workmanship, under normal use and service, for a period of ninety days (90 days) after date of shipment. The Company's obligation under this warranty is limited to repairing or furnishing, without charge, fob point of manufacture, a similar part to replace any part which within one-year after date of shipment is proven to have been defective at the time it was shipped, provided the purchaser has given the Company timely written notice. The Company shall have the option of requiring the return of the defective part, transportation prepaid, to establish the claim. No allowances will be made, or charges accepted, for repairs or alterations performed by or on behalf of the purchaser unless with written consent of the Company. Parts, engines, compressors or other equipment furnished by the Company, but not manufactured by the Company, will carry only the warranty, if any, of the manufacturer and are not warrantied by the Company, and the Company shall have no liability for breach of any warranty by the Manufacturer. THE WARRANTY DESCRIBED IN THIS PARAGRAPH IS EXCLUSIVE AND IS IN LIEU OF ANY OTHER WARRANTY, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO ANY IMPLIED WARRANTY OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE. THE PURCHASER'S REMEDIES ARE LIMITED TO REPAIR OR REPLACEMENT OF THE DEFECTIVE PART AS PROVIDED IN THIS PARAGRAPH. Correction of defects in the manner and for the period of time provided above, shall constitute fulfillment of all obligations and liabilities of the Company to the purchaser, whether based on contract, negligence or otherwise with respect to or arising out of such equipment. The Company reserves the right to make engineering changes, within good engineering practices, at any time on the equipment described herein. IN THE CASE OF ITEMS REQUIRING A "PLANT START-UP" THE WARRANTY PROVIDED IN THIS PARAGRAPH SHALL BE VOID IF THE SERVICES OF A COMPANY SERVICE TECHNICIAN ARE NOT EMPLOYED DURING PLANT START-UP.

V.	LIMITATION OF LIABILITY:

THE COMPANY SHALL NOT BE LIABLE TO PURCHASER FOR LOSS OF PROFITS, SPECIAL, INDIRECT, INCIDENTAL, OR CONSEQUENTIAL DAMAGES ARISING OUT OF BREACH OF THIS AGREEMENT OR OBLIGATIONS UNDER THIS AGREEMENT OR OUT OF WARRANTY, CONTRACT, TORT, OR OTHERWISE. The remedies of the purchaser set forth in this contract are exclusive, and, even if the limited, exclusive remedy provided above should fail of its essential purpose, the liability of the Company with respect to this contract, or anything done in connection therewith, such as, the performance or breach thereof, or from the manufacture, sale, delivery, installation or technical direction of installation, repair or use of any equipment covered by or furnished under this contract whether in contract, in tort, under warranty, or otherwise, shall not exceed the price of the equipment or of the part on which such liability is based.

VI.	LIMITATION OF ACTION:

ANY SUIT BY PURCHASER FOR VIOLATION OF THESE CONDITIONS OF SALE OR BREACH OF WARRANTY MUST BE	BROUGHT WITHIN ONE HUNDRED TWENTY DAYS (120 DAYS) FROM THE	DATE OF DELIVERY OF THE EQUIPMENT TO PURCHASER.

VII. GOVERNING LAW:

The agreement between the Company and the Purchaser shall be governed by and construed in accordance with the laws of the State of Wyoming.

VIII. SHIPPING DATES:

The time for shipment given is approximate and is estimated from the date of receipt of order with complete manufacturing information and approval of drawings as may be necessary. The Company shall not be liable for loss or damage from delay or non-delivery due to acts of civil or military authority, acts of the purchaser, or by reason of "force majeure" which shall be deemed to mean all other causes whatsoever not reasonably within the control of the Company, including but not limited to acts of God, war, riot or insurrection, blockades, embargoes, epidemics,fires, strikes, lockouts, or other industrial disturbances, delays of carriers, and inability to secure materials, labor or manufacturing facilities.

IX.	CANCELLATIONS:

This contract cannot be canceled without mutual agreement between the purchaser and the Company. If such cancellation is agreed upon, purchaser agrees to pay immediately all cancellation charges in accordance with the following:

(A) No order cancellation accepted within 60-days of the scheduled shipping date.

(B) A penalty of 30% of invoice value will be assessed for any cancellation between 60 and 120 days of scheduled shipping date.

(C) A penalty of 20% of invoice value will be assessed for cancellation between 120 and 180 days of scheduled shipping date.

(D) A penalty of 15% of invoice value will be assessed for any cancellation between 180 and 360 days of scheduled shipping date.

X.	INSURANCE:

The purchaser shall bear all risk of loss or of damage to the machinery while being transported and installed and shall provide and maintain adequate insurance against loss or damage by delivery and final payment in an amount fully protecting the Company. Loss or damage by fire or other causes within such period shall not relieve the purchaser from his obligation to pay the purchase price in full.

XI.	TAXES:

The purchaser shall pay to the Company, in addition to the purchase price, the amount of all sales, use, privilege, occupation, excise, or any other taxes, federal, state, local, or foreign which the Company is required to pay in connection with furnishing goods and services to the purchaser.

XII.	INSTALLATION:

Equipment shall be transported, installed and connected at the purchaser's risk and expense.